{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Hoja1","Copiyright"],"not_rendered":{"charts":1,"images":4,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Hoja1","index":0,"n_rows":61,"n_cols":6,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[]
["Po = presión de la cámara del motor."]
["Kn = Klemmung, Kn = Ab /At (Proporción de la superficie del área de combustión vs. el área de la garganta de la tobera)."]
["a = coeficiente de combustión bajo presión."]
["α = factor de la conversión, MPa a Pa (α = 1.000.000)."]
["ρ = densidad de la masa de propelente."]
["c* = velocidad de descarga característica del propelente."]
["n = exponente de combustión bajo presión."]
[]
["Po","Kn",null,"a =",0.00826,"m/s"]
[0,0,null,"α =",1000000]
[0.05391996500278171,10,null,"ρ =",1795,"kg/m3"]
[0.14920751976814017,20,null,"c* =",923.16,"m/s"]
[0.27062516855982305,30,null,"n =",0.319]
[0.41288758170023665,40]
[0.5729771108320209,50]
[0.7488749331636788,60]
[0.9391087489265035,70]
[1.1425439909944193,80]
[1.358272058489918,90]
[1.5855443078783535,100]
[1.823730213512361,110]
[2.0722893901752295,120]
[2.3307520818183187,130]
[2.5987050847057445,140]
[2.8757813027481847,150]
[3.1616518132657307,160]
[3.4560197176607823,170]
[3.758615292261251,180]
[4.069192106302077,190]
[4.387523872628935,200]
[4.71340186257777,210]
[5.046632761545038,220]
[5.387036873249575,230]
[5.734446603107515,240]
[6.088705167380448,250]
[6.4496654867005105,260]
[6.817189231483523,270]
[7.191145993470042,280]
[7.571412562775943,290]
[7.957872293806404,300]
[8.350414546485679,310]
[8.748934191694774,320]
[9.15333117174618,330]
[9.563510108275297,340]
[9.979379951178046,350]
[10.400853663239065,360]
[10.827847935924227,370]
[11.260282932492704,380]
[11.698082055147855,390]
[12.14117173341443,400]
[12.589481231321574,410]
[13.042942471299444,420]
[13.501489872974867,430]
[13.96506020528626,440]
[14.433592450537846,450]

{"sheet":"Copiyright","index":1,"n_rows":9,"n_cols":2,"rows_kept":9,"cut":false,"hidden":false,"merged":[[5,1,6,3]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"Javier E. Fernandez"]
[]
[]
[null,"quimeifc@yahoo.com.ar"]